# Marlin 3D Printer Firmware
![Marlin logo](https://git.trov.ar/trovar/marlin-anet-a8/raw/branch/main/buildroot/share/pixmaps/logo/marlin-250.png)

## Flash instructions

1. Install Anet board definition for Arduino IDE from `./anet-board` ([Source](https://github.com/SkyNet3D/anet-board))
2. Install LiquidCrystal library for Arduino using the IDE library manager
3. Flash selecting `Anet V1.0 (Optiboot)` as board
